|  |  |
| --- | --- |
| Equipment | Centrifuge Non-Refrigerated |
| Business Unit | OR Tambo Chris Hani |
| Req # | 1446906 |
|  |  |
| **Specifications** | **Details** | **Compliant** | **Non-Compliant** |
|  |  |  |  |
| Driver | Brushless induction |  |  |
| Control | Microprocessor |  |  |
| Speed | 3000-5000rpm |  |  |
| Programmability | Pre-set and most recent ,visual digital |  |  |
| Balance detection | Electronic with alarm and cut off |  |  |
| Dimensions | Bench top: 300x 400x 600mm |  |  |
| Run Time | Set and continuous |  |  |
| Decibels | <=60 |  |  |
| Manufacture standards | ISO 13485/9001 |  |  |
| Number of tubes per adaptor per rotor configuration | 48(rotor4 head adaptor with 12 tubes per bucket) |  |  |
| Tube size | 4-13ml |  |  |
| Rotor | Swing head |  |  |
| Adaptor bucket safety | Aerosols-tight |  |  |
| Lid | Lock with safety release |  |  |
| Delivery period | 2-4weeks |  |  |
| Warranty period | Minimum 1 year |  |  |
| Operators manual | Yes |  |  |
| Calibration certificate | Yes |  |  |
| Prevebtative maintenance | Minimum of 1 per year within warrantee period with calibration certificate |  |  |

|  |  |
| --- | --- |
| Laboratory Manager | Winisile Bentswana |
|  |  |
| Signature | wbents |
|  |  |
| Date | 21/11/2024 |
|  |  |
| QAC | Mr Thabede |
|  |  |
| Signature |  |
|  |  |
| Date | 21/11/2024 |