**POCT Site I.T Specifications**

1. 15U Network cabinet (Must Supply Brochure)
2. Cat6 Network Points, 3m Flyleads,  1.2m patch leads (Molex)
3. 3KVA UPS, specs below. Ensure the UPS is connected to the Hospital Generator Power Supply. (Must Supply Brochure)

A list of instructions and instructions

AI-generated content may be incorrect.

1. 24 Port Network switch – Specs below, ensure switch comes with 4 SFP Ports for Fibre connection (Must Supply Brochure)

A close up of a list of information

AI-generated content may be incorrect.

1. Fibre Connection  - (Including all material required to connect both switches)
2. 24 Port patch panel (Cat 6/Molex)
3. All trunking to be 100/100
4. 10 way / 5 way power adapter, installed in the network cabinet and connected to the UPS